Installation steps for windows based silabs connect application

Prerequisites:

* Turn on Bluetooth (In PC) .

Steps:

1. Open folder “**<Release\_Package>/utilities/ble\_provisioning\_apps/windows\_based\_provisioning\_app/”**
2. Run “**install9116sw.ba**t” file to
   1. Ask the user to install **python 3.7.9**
   2. Please make sure enable the "**Add Python 3.7 to PATH**" option and go for installation.

(Make sure to click on “**add path to environment variables**” while installation)

* 1. It also installs required packages (**pillow** and **bleak**).

Graphical user interface, text, application

Description automatically generated

1. After installation is success, Go to folder “**<Release\_Package>/utilities/ ble\_provisioning\_apps /windows\_based\_provisioning\_app/”** and please run “**Silabs\_Connect.py**” in command prompt.

#python **Silabs\_Connect.py** to launch silabs connect windows application.